'{$STAMP BS2}
'{$PBASIC 2.0}

'Program 1

OUTPUT 1
OUT1 = 1
OUTPUT 2
OUT2 = 1
OUTPUT 3
OUT3 = 1
OUTPUT 4
OUT4 = 1

HIGH 5


again:
PAUSE 1000
PULSOUT 1,5000
PULSOUT 2,4000
PULSOUT 3,3000
PULSOUT 4,2000
PULSOUT 5,50000
GOTO again




RETURN